Testing prior knowledge

Title: CORROSION RATES

Measuring the rate of iron corrosion

Choose the correct answer.

1. Dissolve 1.404 g Fe(NH4)2(SO4)2. 6H2O in a 1000 cm3 volumetric flask. What will be the Fe2+ content in 1 cm3 of solution?

a. 1.8 mg

b. 0.2 mg

c. 0.1 g

d. 0.5 mg

2. If the transmission of solution is 50%, the absorbance is…
a. 1.500

b. 0.500

c. 5.72

d. 0.301 

3. Aqueous corrosion of iron requires:
a. H2O

b. O2
c. both

d. air

4. What mass of iron is present in 0.5267 g of ammonium-iron(II) sulfate‑6‑water?
a. 10 mg

b. 75 mg

c. 100 mg

d. 750 mg

Note: answers are given in red. These need to be removed before the test is used.

